**Pursuit Side View Mirrors**

|  |  |
| --- | --- |
| **Part Number** | **Fitment** |
| 18071 | 1.75" Roll Cages |
| 18072 | 2” Roll Cages |
| 18073 | Polaris Pro-Fit Roll Cages |

[Watch the video](http://youtu.be/itz1mmPOwFA" \t "blank): http://youtu.be/itz1mmPOwFA

* The cast aluminum housing can withstand the most extreme punishment.
* Weather sealed caps keep out debris. Color kits available.
* The rubber vibration isolator means a clear image & keeps the mirror from sliding
* Position tension adjustment bolts
* Cast aluminum & steel clamp has low-mass design allowing it to work with virtually any windshield.
* Notched Delrin® detents allow the mirror to fold in when hit and be returned to its original position in one move.
* The adjustable independent glass stays where you set it, keeping riders focused on the trail and not their mirror.
* The Pursuit mirrors are fully adjustable and serviceable. Independent convex safety glass provides a wide viewing angle and can be replaced without having to replace the whole mirror.
* We make good stuff and we stand behind it. All Seizmik mirrors are backed by our Unlimited Lifetime Warranty.

**Weather Seal Caps**

Available in 3 colors\*

|  |  |
| --- | --- |
| Part Number | Color |
| 18074 | Red |
| 18075 | Yellow |
| 18076 | Green |

\*Black comes standard with the mirrors. Color sets sold separately

Updated 2/7/20

* **Cast Aluminum Housing**—Designed to withstand the most extreme punishment
* **Weather Sealed Caps**—Designed to keep out debris (red, yellow, and green color kits available)
* **Rubber Vibration Isolators**—Keeps a clear image and the mirrors from sliding
* **Position Tension Adjustment Bolts**—For keeping your mirror at just the right angle
* **Low Profile Steel Mounting Brackets**—Allow mirrors to work with most any windshield
* **UNLIMITED LIFETIME WARRANTY**

**\*Round Tube shown for illustration.**